Arne Nielsen A/S
Site survey form – heating of large buildings
Infrared heating from Schwank – gas and electric
Fill in the form on site at the customer's premises – it takes 15–20 minutes with a tape measure and a phone. Send the completed form to us by email together with photos and any drawings. You will then receive a sized proposal with layout and bill of materials.
Send to: info@arnenielsen.dk  ·  Fields that are not known can be skipped.
	1. Customer and project


	Company
	

	Address (building location)
	

	Contact person and email
	

	Installer / consultant
	

	Desired start
	

	Date of survey
	



	2. The building


	Length × width (m)
	

	Height to eaves / ridge (m)
	

	Desired mounting height (m)
	

	Roof structure
	☐ Steel   ☐ Timber   ☐ Concrete   ☐ Other: ______

	Can the roof carry suspended loads?
	☐ Yes   ☐ No   ☐ Don't know

	Year of construction
	

	Insulation
	☐ Good   ☐ Average   ☐ Poor   U-values (if known): ______

	Floor
	☐ Concrete   ☐ Other: ______



Doors
	Door no.
	Width × height (m)
	Location (wall)
	How often open?

	
	
	
	

	
	
	
	

	
	
	
	



	Obstructions at ceiling level
	☐ Overhead crane   ☐ Lighting   ☐ Ventilation   ☐ Sprinklers   ☐ Other: ______



	3. Use


	What is the building used for?
	

	Working hours (days and hours per week)
	

	Where do people stand and work?
	



Desired temperature per zone
	Zone
	Area (m²) / location
	Desired temp. (°C)
	Note (e.g. frost protection only)

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



	4. Energy


	Gas available
	☐ Natural gas on site   ☐ Natural gas in the street   ☐ LPG   ☐ No gas

	Electricity (supply, if known)
	

	Current heat source
	☐ Oil   ☐ Gas   ☐ Electric   ☐ Heat pump   ☐ None   ☐ Other: ______

	Approx. annual consumption
	

	Flue possible through
	☐ Roof   ☐ Wall   ☐ Don't know



	5. Requirements


	Budget (if known)
	

	Cooling needed in summer?
	☐ Yes   ☐ No

	Other requirements or comments
	



	6. Attachments – please include


☐ Photos of the interior: ceiling, doors and walls
☐ Drawing or hand sketch with dimensions (feel free to use the last page)
☐ Building records, if available

	Good to know
Gas-fired infrared heating is best suited to buildings with a ceiling height of approx. 4 m or more and access to gas. If the building is lower, or there is no gas, electric infrared heating (eSchwank) or a heat pump may be the right answer – we will assess this based on the form.
The system is sized by the manufacturer's technical department, and the gas-fired radiant heaters are certified under the EU Gas Appliances Regulation (EU) 2016/426.



Sketch of the building – dimensions, doors, zones and desired heater positions
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